DDS

We have two types of DDS (Direct Digital Synthesis) with USB port or Serial port.

Use the right software for programming!

Default Values:

You can use the “Internal Clock Frequency 400 MHz” or “External Clock Frequency: 100 MHz (Input power should be 10 dBm < P < 20 dBm)”.

Input Powers for Divider Setup:

f_in < 150 MHz ⇒ 10 dBm < P < 20 dBm

f_in > 150 MHz ⇒ P ~ 0 dBm

USB-DDS

Software … for USB Type PTB DDS

Umbau zum Frequenzteiler

Anleitung zum Teilerumbau

Datasheet:

Serial-DDS

Software Terminal for Serial Type DDS

Datasheet: