AOM´s

Informations are based on Datasheets found in our office. I did not check if all AOM do excist or are working!

IntraAction:

ASM-1501M3: 150+-40 MHz for 257 nm and 1mm Dia beam: Is in use at SHG 2.

ASM-1501M3: 150+-40 MHz for 257 nm and 1mm Dia beam: Is broken.

ASM-1501LA3: 150+-40 MHz for 266 nm and 1mm Dia beam: Is available.

ASM-852-5: 85+-15 MHz for 326nm and 2mm Dia beam: Is available.

ASM-80: 80+-15 MHz for 440 - 700nm

Neos Technologies:

N35085-0.5: 85 MHz for 400 - 540nm

Isomet:

Isomet 1205C-20: 65 - 95 MHz for 442 - 1060 nm and 2mm Dia aperture: Is available.

Isomet 1205C-20: 65 - 95 MHz for 442 - 1060 nm and 2mm Dia aperture: Is broken.

Isomet 1205C-20: 65 - 95 MHz for 442 - 1060 nm and 0.75mm Dia aperture: Is available.

Crystal Technology:

AOMO 3080-120: 80+-20 MHz for 442 - 633 nm and 2.5mm * 1mm Dia aperture: Is available.

AOMO 3220-120: 220+-60 MHz for 413 nm and 3mm Dia aperture: Is in Use at SHG 1.

AOMO 3350-120: 350 MHz for 488 - 532 nm and 3mm Dia aperture: Is available.

AOMO 3350-120: 350 MHz for 488 - 532 nm and 3mm Dia aperture: Is broken.

AOMO 3080-198: ??? MHz for 1064 nm and 3mm Dia aperture: Is available.

Gooch & Housego:

I-M110-2C10B6-3-GH26: 110 MHz for 400 - 540 nm, Vertical polarization

unknown:

3080-4: ??? MHz for ??? nm and ?mm Dia aperture: The enclosure is missing.

Ther are also Datasheets of other companies like:

IntraAction 3x Model AOM-80, 80+-15 MHz, 440 - 700 nm and 1mm Dia aperture.

Isomet 2x Model 1250C-2, 80 MHz, 442 - 1060 nm and 2mm Dia aperture.

Isomet 1x Model 1250C-2, 200+-50 MHz, 442 - 1060 nm and 0.75mm Dia aperture.

This are not listed yet. Fell free to complete this list!