457 nm-Laser (Wutz)

Operation Values

To Do! Picture!

Edit any other values!

Lasersystem - Typical power values

The system was build by … and is described in his ….

914 nm-Laser

Outputpower after TA: ~ 490 mW

457 nm-SHG

Operation outputpower: ~ 130 mW

Max outpupower: 200 W

Power for photodiode: ~ … müW

AOM´s

Double pass AOM (Wutz)

Power infront the AOM in 1. order: … mW

Power behind the AOM: … mW (efficiency ~ … %)

AOM 1 (Spectroscopy)

Power infront the AOM in 1. order: … mW

Power behind the AOM: … mW (efficiency ~ … %)

AOM 2 (Sisyphus)

Power infront the AOM in 1. order: … mW

Power behind the AOM: … mW (efficiency ~ … %)

Fibers

Wutz

Infront fiber: …

After fiber: … [efficiency ~ … %]

Spectroscopy

Infront fiber: …

After fiber: … [efficiency ~ … %]

Operation power: … mW

Sisyphus

Infront fiber: …

After fiber: … [efficiency ~ … %]

Wavemeter

Infront fiber: …

After fiber: … [efficiency ~ … %]

Wutz-resonator

After cube: … müW

Infront aperture: ~ 350 müW