Clocklaser

ECDL and stabilization

Lasersystem downstairs

Taperea Amplifier (upstairs)

Typical power values

Seedpower: min 10 mW

Outputpower: 800 mW @ 2.2 A

Max outpupower related to the datasheet: 1.5 W @ 3 A

The system was biuld by Sina Malobabic and is described in her diplomathesis.

EYP-TPA-0915-01500-3006-CMT03-0000

SHG

Typical power values

Outputower: ~ 120 mW

Power transfered through the fiber: 20 mW

Power behind the lattice mirror: ~7 - 8 mW

SHG Photodiode is saturated for full Inputpower.

SHG beamprofil has some additional “spots” on one side

SHG beam direction of the blue beam changes with the Inputpower → Adjust at maximal power.