Fiber Comb Control

Start fiber comb control without and after fiber laser program!

To optimize CEO-frequency:

“play” with the arrows in P-Control Laser

To optimize a small Rep-error-signal:

Move in steps Forward/Backward in Repitition Rate Control

possible errors:

If the programm doesn´t start: Maybe COM Port wrong (should be COM1 in device manager)!

Start NI Device Monitor;

if NI card (PCI 6221) is not available: Maybe a Re-Install of NIDAQ helps (in the software/comb folder): enables PCI-6221 card