Fiberlaser

Close the program “Fiber Comb Control” and lock out the CEO- & REP-PID in the rack, otherwise you can´t optimize the comb!

Push Yes

Push OK

If you turn off and on the freuqency comb, then push in the order:

Reset

Auto on

Enable on

The program is done, if all four boxes [Laser on, Modelocked, Autoscramble, Enabled] are green!

For closing the software:

Halt

Freeze

Close the window