Fiberlaser

Close the program “Fiber Comb Control” and lock out the CEO- & REP-PID in the rack, otherwise you can´t optimize the comb!

Push Yes

Push OK

If you turn off and on the freuqency comb, then push in the order:

Reset

Auto on

Enable on

The program is done, if all four boxes [Laser on, Modelocked, Autoscramble, Enabled] are green!

For closing the software:

Halt

Freeze

Now you can optimize CEO-frequency, therefore play with the arrows Stg 1-Stg 4 for the squeezer. Thereby you have to show the CEO-frequency on the Specki and afterwards show the Beat-Signal with 914nm-laser. If one beat is bad, you found a bad modelock point! And don´t forget to optimize the Beat-Signal with 914nm-laser with the PCF and SHG controllers!

Close the window

Possible problems:

If you can´t modelocked the laser. Don´t worry maybe the fs Laser and Amplifier is off. Then push:

Push Laser on

Push Amplifier on