Laser driver

Company: elektronIQ (KMK)

Typ: lasertreiber_v2.3

Link: Lasertreiber

Datasheet: Lasertreiber v2.3

D-SUB pin assignment: D-SUB

The two soldering point next to the label “P3” have to be connected so that the display shows a comma behind the third digit: