Computer-Name: MgControl
OS: Windows 10 Professional x86 (32 bit) - Needed for old NI-DAQ Legacy 7.5 Beta drivers (for the NI PCI cards)
Security questions:
Q: What was your first pet’s name?
A: wutz
Q: What’s the name of the city where you were born?
A: hannover
Q: What’s the first name of your oldest cousin?
A: ernst

######## Fresh installation (Win10 x86 Professional)

Install drivers (D:\Install\Driver\GIGABYTE GA-H170-D3HP)

RapidStorage(v15.9.8.1051) from the file SetupRST.exe or intel website (Don't use old incompatible driver from Gigabyte website)

Realtek

VGA(v21.20.16.4541)

Activate Windows (Run in cmd.exe with admin rights) - Make sure, the current date is correct

(slmgr -ipk W269N-WFGWX-YVC9B-4J6C9-T83GX)

slmgr -skms kms.rrzn.uni-hannover.de:1688

slmgr -ato

Disable automatic updates (Just “show new updates but dont download/install”)
Disable Standby & HardDisk Shutdown
Disable User Account Control (UAC)
Manually set Pagefile to 8096 MB on C:\
Disable hibernate (anyway useless on SSD, eats space and may wear SSD) (Run in cmd.exe with admin rights)

powercfg -h off

Stop C:\Windows\Installer folder to grow beyong good and evil (Run in cmd.exe with admin rights)

reg add HKLM\Software\Policies\Microsoft\Windows\Installer /v MaxPatchCacheSize /t REG_DWORD /d 0 /f

Limit Recyclebin to 1 GB
Rename Windows-Partition to “System”
Disable useless services (services.msc in command-promt)

Superfetch

Windows Defender

Windows Search

Move User Folders (Right-click, Location, Move)

C:\Users\MgControl\Desktop → D:\System\Users\MgControl\Desktop

C:\Users\MgControl\Downloads → D:\Downloads

C:\Users\MgControl\My Documents → D:\System\Users\MgControl\My Documents

C:\Users\MgControl\My Music → D:\System\Users\MgControl\My Music

C:\Users\MgControl\My Pictures → D:\System\Users\MgControl\My Pictures

C:\Users\MgControl\My Videos → D:\System\Users\MgControl\My Videos

C:\Users\MgControl\Saved Games → D:\System\Users\MgControl\Saved Games

Install all latest Windows Updates
CCleaner
FOxitReader/Adobe reader
Ditto
Notepad++
Launchy
Install AFS

KFW 3.2.2

OpenAFS 1.7.1400

Openoffice/Libre office
Mathematica
HardLinkShellExt

Link D:\Daten\Labview to C:\Daten via Symbolic Link

Sophos

RRZN Website… (http://www.rrzn.uni-hannover.de/sophos_download.html)

Install: savw_97_sa_sfx.exe (Sophos EndPoint Offsite installer)

AutoUpdateURL: http://sophosupd2.rrzn.uni-hannover.de/SophosUpdate/CIDs/S002/SAVSCFXP/

Username: savupd1101

Password: uK7md3Pt

######## Backup with Minitool shadow maker free

Install Git and TortoiseGit

Use your institute email and kerberos login credentials the first time it asks for such login details

For more information on how to commit and push files, follow D:\Daten\Readme SVN GIT.txt

CrystalDiskInfo and add to SysTray (for SMART warnings etc)
TightVNC

Client & Server

Server:

Login-PW: ramsey

Admin-Password: ramsey

Server: Uncheck “Accept incoming connections” (not yet using VNC)

Disable Auto-Defrag (so the SSD doesn't wear that fast)
Labview 2012 Fall (from ftp://labview@softdis.uni-hannover.de/, password: Ee2Di7)

NI-Account (if asked):

User: zipfel@iqo.uni-hannover.de

Password: magnesium24

LabView Core

LabView 2012 (already selected)

Signal Express (has to be selected)

Install NI-DAQ (Legacy) 7.5 Beta drivers (“At NI Website. Google for Windows 7 NI-DAQ beta” or search harddisk for “TDAQ750”. OR at “D:\Install\Driver\Nation Instruments\NI-DAQ 7.5 (Legacy)\TDAQ750”)

Be CAREFUL with the next step

Install Device Driver (Feb. 2012) (Download from NI website or use “D:\Install\Driver\Nation Instruments\Device driver Feb 2012\DCD-Feb12-1”)

Uncheck “Modular Instruments” completely so you can also uncheck NI-DAQmx completely (Not doing this will render the NI-DAQ Legacy driver useless)

Additionally to default selection, select:

Timing & Sync (everything)

Reconfigurable I/0

Distributed I/O

Now open Measurement & Automation from Labview

Devices and Interfaces/Traditional NI-DAQ(Legacy) devices

Change Device IDs:

PCI-6602 (8-channel Counter/Timer with Digital I/O): Gerät 3

PCI-6713 (12bit Analog) : Gerät 1

PCI-DIO-32HS (Digital IO): Gerät 2

Set correct Accessory for the Devices in MAX (Properties/Accessory)

PCI-6713: BNC-2110

PCI-6602: BNC-2121

PCI-DIO-32HS: SCB-68

######## Backup with Minitool shadow maker free

Share for D-Drive (Read only)
Share for D:\Public (Read + Write)
Time Watch

ptbtime1.ptb.de

time1.rrzn.uni-hannover.de

TightVNC DFMirage Driver
Install Puresync and configure the correct folders to be backed up to AFS

######## Backup with Minitool shadow maker free