Fiber Comb Control

Name: Fiber Comb Control v0.4.14

First start FiberLaser for better autotuning and afterwards Fiber Comb Control for controlling Repetition Rate Stepper Motor and CEO Tuner

Start fiber comb control without and after fiber laser program!

To optimize CEO-frequency:

“play” with the arrows in P-Control Laser

To optimize a small Rep-error-signal:

Move in steps Forward/Backward in Repitition Rate Control

In Lockbox Rep Rate is locked disabled (red), because it is not connected to the menlosystem electronics.

possible errors:

If the programm doesn´t start: Maybe COM Port wrong (should be COM1 in device manager)!

Start NI Device Monitor;

if NI card (PCI 6221) is not available: Maybe a Re-Install of NIDAQ helps (in the software/comb folder): enables PCI-6221 card