Fiberlaser

Software Installation

Verion name: FiberLaserv6.9

Manual: fiberlaser-v6.9.pdf

First start FiberLaser for better autotuning and afterwards Fiber Comb Control for controlling Repetition Rate Stepper Motor and CEO Tuner

Close the program “Fiber Comb Control” and lock out the CEO- & REP-PID in the rack, otherwise you can´t optimize the comb!

Push Yes

Push OK

If you turn off and on the freuqency comb, then push in the order:

Reset

Auto on

Enable on

The program is done, if all four boxes [Laser on, Modelocked, Autoscramble, Enabled] are green!

For closing the software:

Halt

Freeze

Now you can optimize CEO-frequency, therefore play with the arrows Stg 1-Stg 4 for the squeezer. Thereby you have to show the CEO-frequency on the Specki and afterwards show the Beat-Signal with 914nm-laser. If one beat is bad, you found a bad modelock point! And don´t forget to optimize the Beat-Signal with 914nm-laser with the PCF and SHG controllers!

Close the window

Possible problems:

If you can´t modelocked the laser. Don´t worry maybe the fs Laser and Amplifier is off. Then push:

Push Laser on

Push Amplifier on

If the “Scramble Settings arrows” don´t move and the step width are 0. Than change the “step width” from 0 to 3 or 5. Afterwards push the “ Send” button.