Tracker

Welche Tracker haben wir → Tabelle

How to set a tracker?

Find out the input frequency with a spectrum analyzer

Turn on the tracker (K+K counter and tracker have different pin assignments !)

Turn the gain down to 0

View the monitor output or A/B output frequency on the spectrum analyzer (Maybe too strong signal, dBm)

Turn the frequency by means of the VCO rotary knob to the required frequency

Now plug in the RF signal in the RF signal input

Turn the gain up until you can see a better signal

Done

Controversial discussion: Some people use the integrator and some people not. Usually we don´t use the integrator. If you want to use it, aktivate the integrator after step 7).

The advantage of using the integrator: The Tracker stay phase stable!

Without the integrator, there may be a deviation of 1 Hz

The integrator is used as lowpass

If the tracker doesn´t work, turn off and on the complete power supply.