EOM and AOM Box

Idea: <fc #ff0000>PAPER FOR EOM/T CONTROL</fc>

Advantages

easy to handle

robust

mechanics/temperature stabil

active control of the temperature of the EOM

Components

Optics

1x Fiber-AOM

1x Fiber-EOM

1x Fiber-Coupler/Splitter

2-3x Fiber-rewinder (=Aufwickler)

-

Mechanics

Alu-Box (Typ: 01182810/A131)

Breadboard

Mount for AOM (Material: Alu)

Mount for EOM (Material: Alu, Cupper, Teflon, …)

Electronics

2x SMA connectors for RF-freqeuncy

1x BNC connector for out-of-loop temperature measurement

1x Sub-D-9-Male connector for temperature controlling

2x Peltier elements (Typ: QC-K03504T125, 189186 from Quick-Coo)

Electronic connections

Sub-D-9

Typ: Male

Normal Sub D-9 Connector

Pin-assignment PTB-styl

Pin	Name
1	-
2	-
3	-
4	NTC (for AD590 +)
5	NTC (for AD590 -)
6	Peltier -
7	Peltier +
8	-
9	-

Possible setup