EOM and AOM Box

Idea: <fc #ff0000>PAPER FOR EOM/T CONTROL</fc>

OBJ
1	iqo_baugruppe_280x180_final.pdf
2	iqo_gehaeuse_280x180.pdf
3*	iqo_boden_280x180.pdf
4	iqo_aluplatte_aom.pdf
5	iqo_aluplatte_eom.pdf
6	iqo_teflon_abstandshalter.pdf
7	iqo_kupferplatte.pdf

Advantages

easy to handle

robust

mechanics/temperature stabil

active control of the temperature of the EOM

Components

Optics

1x Fiber-AOM

1x Fiber-EOM

1x Fiber-Coupler/Splitter

2-3x Fiber-rewinder (=Aufwickler)

Mechanics

Alu-Box (Typ: 01182810/A131)

Breadboard

Mount for AOM (Material: Alu)

Mount for EOM (Material: Alu, Cupper, Teflon, …)

*Annotation

please view the the notes on verbal agreements on the technical drawing 3 !

Die Anfertigung eines Bodens mit Schraubverbindungen an Laschen zur Nutzung der vorhandenen Bohrungen, erwies sich als zu Komplex. Die Realisierung einer 100%igen Ebenheit und somit thermischen Kontaktes der Flächen, konnte nicht gewährlistet werden. Hinzu kam die Berücksichtigung wirkender Zugkräfte, die einem thermischen Kontakt entgegengewirkt hätten. Daraufhin entschied man sich für Schraubverbindungen mittels Senkkopfschrauben im Boden der Alubox.

Electronics

2x SMA connectors for RF-freqeuncy

1x BNC connector for out-of-loop temperature measurement

1x Sub-D-9-Male connector for temperature controlling

2x Peltier elements (Typ: QC-K03504T125, 189186 from Quick-Coo; Datasheet: 189186-da-01-de-peltier_element_3504.pdf)

2x 10kOhm NTC (Typ: Epcos B57861S)

Cables for NTC´s 0.25mm^2 (max. 4A)

Heat-conducting paste between peltier elelements to Al-mount and peltier elements to cupper mount

NTC´s cables are twisted and have a shield, which is connected to earth

Electronic connections

Sub-D-9

Typ: Male

Normal Sub D-9 Connector

Pin-assignment PTB-styl

Pin	Name	Color(s)
1	-	-
2	-	-
3	-	-
4	NTC (for AD590 +)	Blue
5	NTC (for AD590 -)	Green
6	Peltier -	Grey, Yellow, Pink
7	Peltier +	Red, Brown, White
8	-
9	-