Fiber-Components

How to work with fiber modulators:

english: Modulatorfibel_english

german: Modulatorfibel_german

Fiber EOM

Company: Jenoptik

Do not apply voltages higher than 40V peak-peak to RF input.

Typ: PM1550

Center wavelength: 1550 nm

Insertion loss: 3.0 dB

Electonic connector: SMA, Inputimpedanz: 50 Ohm

U_pi@1kHz: 8.5 V

Fiber-typ: PM

Fiber-connector: FC/APC

Fiber length: 1m

Crystall: Lithiumniobat (Info_crystall)

Max optical input power: 300mW cw

Datasheet:

supplied:

german: Datasheet Fiber-Eom_german

english: Datasheet Fiber-Eom_english

Fiber Coupler

50/50

Company: Opneti

Typ: CS-PS-A-2×2-1550-50/50-900-5-0.25-FA-3×54

Type: PS=PM Fused Coupler

Grade: A=Grade

Port Type: 2×2

Wavelength: 1550

Coupling Ratio: 50/50

Pigtail Type: 900=900um Loose Tube

Fiber Type: 5=Panda Fiber

Length: 0.25m

Connector: FA=FC/APC

Package: φ3.0×54

Datasheet: Datasheet Fiber-coupler_50/50_Opneti

Test report: