Fiber-Components

How to work with fiber modulators:

english: Modulatorfibel_english

german: Modulatorfibel_german

Fiber AOM

Company: AMS Technologies AG, Gooch & Housego Torquay

RF power: 0.4 W. Absolute maximum rating. Higher power will cause damage.

Typ: SFO4504-T-M080-0.5C8J-3-F2P

Fiber-coupled acousto-optic modulator, model Fibre-Q http://www.amstechnologies.com/products/optical-technologies/components/optics/acousto-optics/view/fibre-coupled-acousto-optic-modulators/

Material: Amtir

Wavelength: 1550 nm

Operation frequency: +80 MHz

Polarisation maintaining fiber

Fibre length: 0.3M

Gibre-connector: FC/APC

Datasheet:

from AMS technologies: Datasheet_Fiber-AOM-G&HT_AMS

from G&HT internetside: Datasheet_Fiber-AOM-G&HT_G&HT

Testreport: Fiber-AOM-Testreport-G&H

Company: Laser2000, Brimrose

RF power: <0.5 W. Absolute maximum rating. Higher power will cause damage.

Typ: BRI-AMF-80-4-1550-2FP-FC/APC-0.3

Fiber-coupled acousto-optic modulator,

Material: Amtir

Wavelength: 1550 nm

Operation frequency: +80 MHz

Polarisation maintaining fiber

Fibre length: 0.3M

Gibre-connector: FC/APC

Datasheet: Datasheet_Fiber-AOM-Brimerose

Fiber EOM

Company: Jenoptik

Do not apply voltages higher than 40V peak-peak to RF input.

Typ: PM1550

Center wavelength: 1550 nm

Insertion loss: 3.0 dB

Electonic connector: SMA, Inputimpedanz: 50 Ohm

U_pi@1kHz: 8.5 V

Fiber-typ: PM

Fiber-connector: FC/APC

Fiber length: 1m

Crystall: Lithiumniobat (Info_crystall)

Max optical input power: 300mW cw

Datasheet:

german: Datasheet Fiber-Eom_german

english: Datasheet Fiber-Eom_english

supplied:

Fiber FRM

Company: Laser2000, General Photonics

Typ: NFRM-15-FCA

Operating Wavelength: 1550 nm

Operating Bandwidth: ±50 nm

Insertion Loss:

typical: 0.3 dB

max: 0.5 dB

Faraday Rotation Angle: 90 degrees

Rotation Angle Tolerance (Center Wavelength at 23 °C): ±1 degree

Rotation Angle Wavelength Dependence: ±0.12 degree/nm

Rotation Angle Temperature Dependence: ±0.12 degree/°C

Reflection Polarization Dependence: 0.5% max.

Optical Power Handling: 300 mW min.

Operating Temperature 0 to 70 °C

Storage Temperature: -40 to 85 °C

Fiber Type: SMF-28

Dimensions: Ø 9.5 × 50 mm (NoTail)

Datasheet: frm.pdf

Fiber Coupler

50/50

Company: Opneti

Typ: CS-PS-A-2×2-1550-50/50-900-5-0.25-FA-3×54

Type: PS=PM Fused Coupler

Grade: A=Grade

Port Type: 2×2

Wavelength: 1550

Coupling Ratio: 50/50

Pigtail Type: 900=900um Loose Tube

Fiber Type: 5=Panda Fiber

Length: 0.25m

Connector: FA=FC/APC

Package: φ3.0×54

Datasheet: Datasheet Fiber-coupler_50/50_Opneti

Test report: