Incoupling breadboard components

Fiber collimator

Company: Schäfter+Kirchoff http://www.sukhamburg.com/products/Fiber_collimators_60FC-_.html

Model: 60FC-4-A2.7-45

Housing diameter: 12mm

Focal length: 2.75mm

Coating: AR 1300-1750nm Coating sheet

NA: 0.55

Connection: FC/APC

Schrägorientierte Koppelachse

Integral focussing

Amagnetic collimators made from titanium on request

Infrared optics made of Chalcogenide glass for wavelengths > 1000 nm (see Technical Data, lens designed for λ = 2.5 μm)

2D-drawing: 970920020518.pdf

Free beam optical isolator

Company: Nortus Optronic GmbH, Isowave

Model: I-15UHP-4

Serial Number: 45830

Wavelength: 1515-1585nm

Clear Aperture: 4mm

Isolation

Typ: 75dB

Minimum: >60dB

testet by 1550nm: 71dB

Transmission: 83% (90% Typ)

Ambient Temp: 23 °C

Insertion loss: 0.5dB

Test report

Datasheet

Length: 42.3mm

Diameter: 19mm

DS Polaristaor

Company: Qioptiq Phtonics GmbH Link: http://photonics.specpick.com/products/polarizers/edmund-optics-inc/36-434-g335753000

Article number: G335-753-000

Dimensions h=L1=L2: 10x10mm

Tolerance:

High h: -0.09mm

L1=L2: ±0.2mm

Wavelength: 1100-1700nm

Datasheet

Special beamsplitter coatings yield highly polarized transmitted beams

Combine extreme spectral bandwidth with superb extinction ratio and transmittance

Extinction ratio transmission > 10,000:1 (ΦTp : ΦTs) at ± 2°

No angular or lateral deflection of transmitted beams

Less than λ/4 wavefront distortion at 633 nm

Broadband coated with ARB2

Tp > 90%

Damage thresholds: > 2 kW/cm2 cw (488/514 nm)

Damage thresholds: > 200 mJ/cm2 for pulses of 10 ns (1064 nm)

Damage thresholds: > 28 mJ/cm2 for pulses of 280 fs (850 nm, 20 Hz)

Mirror holders

Company: Thorlabs

Typ: Polaris-K05S1 https://www.thorlabs.com/thorproduct.cfm?partnumber=POLARIS-K05S1

2-Adjuster Hex-Driven Design https://www.thorlabs.com/newgrouppage9.cfm?objectgroup_id=10690&pn=POLARIS-K05S1

Designed for use with Ø1/2“ Optics

±5° Mechanical Angular Range

~11 mrad/rev Resolution

datasheet: polaris-k05s1-specsheet.pdf

Mirrors

Company: Thorlabs

Mirror Sepcifications

Typ: BB0511-E04 https://www.thorlabs.com/thorproduct.cfm?partnumber=BB0511-E04

Diameter: 12.7mm (1/2”) +0.0 mm / -0.1 mm

Thickness: 6.0 mm (0.24“) ±0.2 mm

Coating Specifications

Broadband Coatings: 1280-1600 nm

Ravg > 99% for S- and P-Polarizations for Angles of Incidence from 0 to 45°

Substrate material: Zerodur

Zerodur®'s coefficient of thermal expansion is 0 ± 0.100 x 10-6 /°C, which is significantly smaller than the value for fused silica, 0.55 x 10-6 /°C

Damage Threshold: 2.5 J/cm2 (1542 nm, 10 ns, 10 Hz, Ø0.181 mm)

Linear Stages

Company: Newport

Typ: M-DS25-X https://www.newport.com/p/M-DS25-X

Axes of Travel: X

Maximum Stage Travel: 6.35 mm

Load Capacity: 45 N

Material: Aluminum

Centered Load Capacity with BM Micrometer: 11 N

Platform Size: 25 x 25 mm

Sensitivity: 1 µm

Beamsplitter Cube

Company: Thorlabs

Typ: BS012 https://www.thorlabs.com/thorproduct.cfm?partnumber=BS012

Size: 10.0 x 10.0 mm

No Polarization

Splitting: 50:50

Wavelength: 1100 - 1600 nm