19.10.2016

I cleaned the vacuum chamber

I tested the M6 holes from vacuumchamber all threads are deep enough!

2x M4-breadboards (Incouple and otcouple) and there spacers are done!

I assembled the mounting with vitonballs and zerodur rods. We need two vitonballs of each metal sheet side. Otherwise the mounting is to wobbly! 8x new sinkings for the vitonballs!