02.11.2016

8x sinkings for the vitonballs in each panel:

We measured the diameter of the glasballs and saw an inaccuracy of 80mm +/- 20müm. Therefore we put the balls in a 5mm test-hole and measured the ball-high in different position with the CNC-maschine:

After the “ball-high-measurement”, we calculated the mean value and drilled again test-holes, for example “Kugel 1” 5mm + 19.4müm, and measured again. We saw a really nice result! After a 1cm test-milling and a good result, we milled in the mounting-breadboard:

We build everthing together and measured the high of the mounting on different places with a provisional result of +/- ~80müm: