ULE-compensations-rings

Company: Coastline Optics, Inc.

Quotation: q14-2520_university_of_hannover.pdf

Dimensions:

Diamater: 25.4mm +0.0 / -0.1 mm Ø

Inside diameter: 7.0+/-0.2 mmID

Thickness: 6.30 mm+/-0.2mm

Configuration: Plano/Plano

Polish bothsides flat to 0.25waves P-V @ 633nm,suitablefor optical contacting.

Material: PremiumGrade ULE

We bought 12.