Vacuum

Bake out

We use the temperature monitoring design, made by E. Wodey, for the out of loop measurements during the out baking.

Talk by E. Wodey for the explanation of the monitoring system:2016-08_geoq_ctp_ew.pdf

Box-design made by S. Sauer:

Bake out list

Item	Maximum temperature
Mounting for the spacer
Zerodur rods
Viton balls
Glas balls
Heat shields
Screws from the mounting
Windows (inside and outside the vacuumchamber)
Window holder
ULE rings
Vacuum chamber
CF Cupper rings
CF Flanschkit
IGP
IGP cable
Vacuum pressure sensor
Vacuum pressure sensor cable
Angle valve
Sub-D Socket
CF-Kreuz
Indium wire
Indium foil
Capton wires
Crimp pins
Peltier-elements
NTC Sensors
Faraday rotator
Glue from faraday rotator
ULE Spacer
Mirrors

Bake out Protocol

Summary of information:

Agilent: “Die einzigen Einflussgrößen auf die Stabilität des Druckes sind Gaslast und Ausgasung (eigentlich auch zur Gaslast gehörend).

Ich sende Ihnen nochmal den entsprechenden Katalogteil. Hier kann man schon vieles nachlesen allgemein zum Betrieb.” agilent_catalog_06_ion_section_120.pdf

Test report scan copy for vacuum compatible isolators: test_report_scan_copy_for_vacuum_compatible_isolators.pdf