TracerDAQ

DAQ Hardware settings

Optimum: +/- 2V. If there is more voltage, then are the resolution of the fluctuation bad.

You can change the time-range in the program TracerDAQ

Software settings

Select Strip Chart

Push Run

You can change the range under: Edit → Scan Rate/Trigger Settings

Push OK

The memory will be very fast full for high scan ranges!

You have to set the DAQ Range/Mode (=Input Voltage) to the right value!

In this window, you can see the error messages, like not connected!

Push Play/Start

Channels on RedLab-Card:
0: R1 Inner T OOL
1: R2 Inner T OOL
2: R1 PDH Out
3: R1 Intens Out
4: R2 PDH Out
5: R2 Intens Out
6: R1 Vacuum
7: ECDL