457 nm-Laser (Wutz)

Lasersystem - Typical power values

The system was build by Toptica (TA-SHG 110)

914 nm-Laser

Outputpower after TA: ~ 490 mW

457 nm-SHG

Operation outputpower: ~ 130 mW

Max outpupower: 200 mW

AOM 1 (Transfer-Fiber)

Power infront the AOM: ~ 117 mW

Power behind the AOM in 1. order: ~ 35 mW

Wutz Resonator Fiber

After fiber: ~ 300 µW

Infront of iris next to resonator: ~ 200 µW