Fiber boxes 360x160

technical drawings: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 360×160

Components

Optics

Mechanics

Alu-Box (Typ: ALS01135 - Best.Nr. M01163609)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

Electronics

6x SMA connectors for

1x BNC connector for

4x fiber conectors (Typ: )

4x fiber conectors (Typ: )

Fiber boxes 200x139

technical drawings: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 200×139

Components

Optics

Mechanics

Alu-Box (Typ: ALS01115 - Best.Nr. M01142009)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

Electronics

4x SMA connectors for

1x BNC connector for

4x fiber connectors (Typ: ) on two opposite sides