Fiber boxes 360x160

technical drawings for Inventor2018: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 360×160

technical drwaing.pdf
Alu-Box	alugehaeuse_360x160.pdf
Alu-base	made to match without drawing

Components

Optics

Mechanics

Alu-Box (Typ: ALS01135 - Best.Nr. M01163609)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

Electronics

6x SMA connectors for

1x BNC connector (Typ: 1426195 Thorlabs) for

4x fiber conectors (Typ: )

4x fiber conectors (Typ: )

Fiber boxes 200x139

technical drawings: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 200×139

technical drwaing.pdf
module	alugehaeuse_200x139_-_baugruppe.pdf
Alu-box	alugehaeuse_200x139.pdf
Alu-base	made to match without drawing
Alu-board for AOM	iqo_aluplatte_aom_2.pdf

Components

Optics

Mechanics

Alu-Box (Typ: ALS01115 - Best.Nr. M01142009)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

Electronics

4x SMA connectors for

1x BNC (Typ: 1426195 Thorlabs) connector for

4x fiber connectors (Typ: ) on two opposite sides