Fiber boxes 360x160

technical drawings for Inventor2018: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 360×160

technical drwaing.pdf
Alu-Box	alugehaeuse_360x160.pdf
Alu-base	made to match without drawing*

Components

Optics

Mechanics

Alu-Box (Typ: ALS01135 - Best.Nr. M01163609)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

* Annotation

Unordered List Itemplease view the the notes on verbal agreements on the technical drawings iqo_boden_280x180.pdf!

Die Anfertigung eines Bodens mit Schraubverbindungen an Laschen zur Nutzung der vorhandenen Bohrungen, erwies sich als zu Komplex. Die Realisierung einer 100%igen Ebenheit und somit thermischen Kontaktes der Flächen, konnte nicht gewährlistet werden. Hinzu kam die Berücksichtigung wirkender Zugkräfte, die einem thermischen Kontakt entgegengewirkt hätten. Daraufhin entschied man sich für Schraubverbindungen mittels Senkkopfschrauben im Boden der Alubox.

Electronics

6x SMA connectors for

1x BNC connector (Typ: 1426195 Thorlabs) for

4x fiber conectors (Typ: )

4x fiber conectors (Typ: )

Fiber boxes 200x139

technical drawings: \\afs\iqo.uni-hannover.de\user\jwolf\work\Resonator\Alugehäuse\Alugehäuse 200×139

technical drwaing.pdf
module	alugehaeuse_200x139_-_baugruppe.pdf
Alu-box	alugehaeuse_200x139.pdf
Alu-base	made to match without drawing*
Alu-board for AOM	iqo_aluplatte_aom_2.pdf

Components

Optics

AOM (Typ: …)

Mechanics

Alu-Box (Typ: ALS01115 - Best.Nr. M01142009)

for thermal contact was milled of the painted surface on the inside and outside of the bottom

Alu-base to allow to use optical components, while thermal contact is assured

for fastening box and base are used four screw connections

Electronics

4x SMA connectors for

1x BNC (Typ: 1426195 Thorlabs) connector for

4x fiber connectors (Typ: ) on two opposite sides