List of Computer-Programs

Save a backup file from each program in AFS!
Name	Description	Computer	Information
TEC Service XY	TEC Control Sofware	“	Meerstetter Control Software for ECDL baseplate, active shieldings of resonators R1 and R2
Allan-Live with time graph	-	”	-
TracerDAQ	RedLab Card Counter	ResLab	Can count Voltages; Limited Capacities / Time;
RbMon	Rubidium clock software	“	-
Net View	GPS receiver	”	Control software for GPS signal.
Fiber Comb Control	…	“	This Software can control Repetition Rate Stepper Motor and CEO Tuner
FiberLaser	First start this	”	First start this, better Autotuning
Kamm-Frequenzneu kombiniert.nb	-	“	-
allen-combined	-	”	-
Spyder	Pyhton Compiler	“	Code for Einstein-Telescope
Pyhtonberechnungen von und mit Schlippi Folder	-	”	-
K&K FXE / FXQE80	Counter	“	Maximal 8 Com Ports
KK FXE Folder	Folder of Counter	”	Counter Daten werden hier gespeichert
…	…	…	…
…	…	…	…
Monitor VCH-1006	Control Software for H-Maser	ResLab Maser	one entry is always red! Andreas Bauch doesn´t know the reason, but it´s okay!
[DDS USB	Programming the USB-DDS	ResLab Maser	-
USB Serial	Programming the USB-Serial	ResLab Maser	- okay!
…	…	…	…
Highfinesse Wavemeter WS/6-200	Wavemeter	ResLab Mobil	Push the “Start Measurement” button
Laser Frequency ResLab.vi	Wavemeter	“	Shows Laser Frequency, also for Atom Lab
K&K FXE / FXQE80 (currently not in use!)	Counter	”	Default Settings: 8 Com Ports, Trimmer: Auto Trimmer, Measurement Method: Phase; Push buttons before measurement to erase RAM: Clear Buffer, Reset; Start Measurement via Häckchen setzen auf frequency;
KK FXE Folder (currently not in use!)	Folder of Counter	“	Counter Daten werden hier gespeichert
…	…	…	…