List of Computer-Programs

Save a backup file from each program in AFS!
Name	Description	Computer	Information
TEC Service XY	TEC Control Software	ResLab	Meerstetter Control Software for ECDL baseplate, active shieldings of resonators R1 and R2
Allan-Live with time graph	-	-
TracerDAQ	RedLab Card Counter	Can count Voltages; Limited Capacities / Time;
RbMon	Rubidium clock software	-
Net View	GPS receiver	Control software for GPS signal.
FiberLaser	Comb	First start this, better Autotuning
Fiber Comb Control	Comb	Second! This Software can control Repetition Rate Stepper Motor and CEO Tuner
Kamm-Frequenzneu kombiniert.nb	-	-
allen-combined	-	-
Spyder	Pyhton Compiler
Pyhtonberechnungen von und mit Schlippi Folder	-	-
K&K FXE / FXQE80	Counter	Maximal 8 Com Ports
KK FXE Folder	Folder of Counter	Counter Daten werden hier gespeichert
…	…	…	…
…	…	…	…
Monitor VCH-1006	Control Software for H-Maser	ResLab Maser	one entry is always red! Andreas Bauch doesn´t know the reason, but it´s okay!
DDS USB	Programming the USB-DDS	-
USB Serial/Terminal	Programming the USB-Serial	-
…	…	…	…
Highfinesse Wavemeter WS/6-200	Wavemeter	ResLab Mobil	Push the “Start Measurement” button
Laser Frequency ResLab.vi	Wavemeter	Shows Laser Frequency, also for Atom Lab
K&K FXE / FXQE80 (currently not in use!)	Counter	Default Settings: 8 Com Ports, Trimmer: Auto Trimmer, Measurement Method: Phase; Push buttons before measurement to erase RAM: Clear Buffer, Reset; Start Measurement via Häckchen setzen auf frequency;
KK FXE Folder (currently not in use!)	Folder of Counter	Counter Daten werden hier gespeichert
…	…	…	…