Mains filter

Application: Suppression of electrical network disturbances.

Mains filter (max. 6A, 230V): 6EMC1 - F8127

Datasheet_6EMC1_F8127

Customer drawing

Safety fuse: 5A

“Measurement point for Current Box”