Net View

“Connection”-window:
“GPS receiver”-button must be selected.
Push “connect”-button.
“Receiver”-window:
The “Measurements”-button/setting shows the coordinates of the satellits.
The “Skyplot”-button/setting shows the connections with the satellites and the names.
The “Skyplot”-button/setting