Jour Fixe

SS, WFP, PG

Atomslab

AC was fixed by the 4440 guys → filter has to be changed once a year

Quench

The alignment of the fiber from the laser further dropped to 570 mW out of 1400 mW.

Alignment of AOM in progress

PTB/Meta-mirror

Reflectivity of Meta-mirror was measured to be 99.8x% via Ring-Down

Measurement of transmission is planned (preperation in progress)

(time-consuming) Tender-process for Wavemeter