ResLab

Installation procedure

1. Install windows

2. Install RAID system in BIOS

https://www.asus.com/de/support/FAQ/1007642/

3. Install drivers

Intel® Optane™ Memory and Storage Management from Microsoft store

https://www.microsoft.com/de-de/p/intel-optane-memory-and-storage-management/9mzng5hzwz1t?activetab=pivot:overviewtab

Install Intel-Driver and Support Assistant

Other Drivers for Mainboard (Always the latest!):

Date: 02.2020:

https://www.asus.com/de/Motherboards/PRIME-H370-PLUS/HelpDesk_Manual/

VGA (Version 26.20.100.7210)

Audio (Version 6.0.1.8339)

LAN (Version 10.31.828.2018)

Chipset (Version 1914.12.0.1256)

4. Activate Windows

Run in cmd.exe with admin rights

Make sure, the current date is correct

RRZN: https://www.luis.uni-hannover.de/kms.html

slmgr -skms kms.rrzn.uni-hannover.de:1688

slmgr -ipk W269N-WFGWX-YVC9B-4J6C9-T83GX

slmgr -ato

5. Windows/Computer Settings

Disable automatic updates

Just “show new updates but dont download/install”

“Windows” + “R” → services.msc

“Windows Update” deaktivieren

Disable Standby & HardDisk Shutdown

Manually set Pagefile to 8096 MB on C:

https://www.windowscrush.com/moving-windows-pagefile-to-another-drive.html

Disable hibernate

anyway useless on SSD, eats space and may wear SSD

Run in cmd.exe with admin rights

powercfg -h off

Stop C:\Windows\Installer folder to grow beyong good and evil

Run in cmd.exe with admin rights

reg add HKLM\Software\Policies\Microsoft\Windows\Installer /v MaxPatchCacheSize /t REG_DWORD /d 0 /f

Limit Recyclebin to 1 GB

Rename Windows-Partition to “System”

Disable useless services (services.msc in command-promt)

Windows Search

Move User Folders (Right-click, Location, Move)

C:\Users\ResLab-Main\Desktop → D:\System\Users\ResLab-Main\Desktop

C:\Users\ResLab-Main\Downloads → D:\Downloads

C:\Users\ResLab-Main\My Documents → D:\System\Users\ResLab-Main\My Documents

C:\Users\ResLab-Main\My Music → D:\System\Users\ResLab-Main\My Music

C:\Users\ResLab-Main\My Pictures → D:\System\Users\ResLab-Main\My Pictures

C:\Users\ResLab-Main\My Videos → D:\System\Users\ResLab-Main\My Videos

C:\Users\ResLab-Main\Saved Games → D:\System\Users\ResLab-Main\Saved Games

Install german language

Create new “Install” folders in D and safe each .exe in there:

D:\Install

D:\Install\Motherboard Drivers

D:\Install\Software_normal for “normal” computer software

D:\Install\Software_ResLab for “special” software of the Lab

Deinstall Software:

One Drive

Dateiendungen anzeigen:

Öffnen Sie irgendeinen Ordner.

Klicken Sie im oberen Bereich auf den Reiter „Ansicht“.

Wählen Sie hier den Bereich „Ein-/ausblenden“ aus und setzen Sie einen Haken unter „Dateinamenerweiterungen“.

Share for D-Drive (Read only)

Share for D:\Public (Read + Write)

Make hidden files and folders visible

Install all latest Windows Updates

6. Install Software

Mozilla Firefox

Install AddblockPlus

Sophos → RRZN: https://www.luis.uni-hannover.de/antiviren.html

Time Watch → https://www.blue-series.com/en/products/time-watch/

Server: ptbtime1.ptb.de

Server selbst hinzufügen: time1.rrzn.uni-hannover.de

AFS → https://iqwiki.iqo.uni-hannover.de/doku.php?id=it:configuration_stuff:connectafs:start

Version: afs_iqo_1.7.33.zip

CCleaner

Notepad++

Libre office

FoxitReader

CPU-Z for stress test of CPU

Launchy

Ditto

Mathematica → https://iqwiki.iqo.uni-hannover.de/doku.php?id=main:mathematica

Install first Git and than TortoiseGit

Use your institute email and kerberos login credentials the first time it asks for such login details

MiniTool ShadowMaker Free

7. Backup with Minitool shadow maker free

from C to D in D:\backupdata

8. Install Software

CrystalDiskInfo (Version: 8.4.0)

add to SysTray (for SMART warnings etc)

TightVNC (Version 2.8.27)

Client & Server

Server:

Login-PW: HMaser

Admin-Password: HMaser

Server: Uncheck “Accept incoming connections” (not yet using VNC)

Puresync

configure the correct folders to be backed up to AFS

9. System Restore with windows

10. Copy old Data from other Hard drives

Do not forget to sort!

11. Install drivers for the printers

under \\printserv

login: IQO\afsusername + afs password

prn-1101-001-d123a-1 for color

https://iqwiki.iqo.uni-hannover.de/doku.php?id=groups:fwj:physiqo2019:sonstiges:farbe_drucken

prn-1101-003-d323-1 for black/white

12. Required software for ResLab

Labview 2012 Fall for Wavemeter-Software and Monitoring for Meerstetter & RedLab-Card

ftp://labview@softdis.uni-hannover.de

User: labview

Passwort: Ee2Di7

NI-Account (if asked):

User: zipfel@iqo.uni-hannover.de

Password: magnesium24

(maybe) Labview 2011 for Comb (?)

File name: LVRTE2011fstd

Ni-drivers for Comb

File name: NIDAQ1600f0Config

FiberLaser

Fiber Comb Control

Highfinesse Wavemeter WS/6-200

Wavemeter-Labview-Software

TracerDAQ

RbMon

TEC Service XY

K&K FXE / FXX_App 1.4 + put K+K_Counter_Data on desktop

stable32

Strahl.exe

13. Software should start automatically by turning on the pc

Autostart

go to Taskmanager

go to Autostart

right click to activate software

To add programs to the autostart, proceed as follows:

Press “Win” + “R” and enter the command shell:startup.

The autostart folder opens. You add more applications by creating a shortcut to the original file in the startup folder. To do this, drag the file into the autostart folder while holding down the right mouse button and then release the button. Select “Create shortcuts here”.

After a Windows restart, the new programs should be started during the autostart

Activate the following software:

Network Identity Manager

HighFinesse wavemeter

Wavemeter ResLab.exe

FXX_App

14. Create shortcuts on the desktop

Dieser PC (folder)

AFS (folder)

Mg-AFS (folder)

FiberLaser

Fiber Comb Control

HighFinesse Wavemeter

Wavemeter ResLab.exe

FXX_App

Counter_Data (folder)

TEC Service

R1

R2

ECDL

put this Mathematica files to desktop:

Allan-Live with time graph

Kamm-Frequenzneu kombiniert

allen-combined

Allan-Live 1.2

Allan-Live 1.2 - USB

Virtual Beat

VirtualBeat_DDSDivider_Error

InstantDrift

PTB Laser Frequenz

PTB Laser Frequenz 1703test

15. Backup with Minitool shadow maker free

Old software under windows 7

Name	Description	Information
NetView	GPS receiver Pyhton Compiler	Control software for GPS signal.
Spyder	Programming software, for expample: Code for Einstein-Telescope
USB Serial/Terminal	Control Software for H-Maser Programming the USB-DDS Programming the USB-Serial

Hardware of ResLab

Mainboard: ASUS Prime H370-Plus

CPU: A0148063 – Intel Core i7-8700, 6x 3.20GHz, tray, Sockel 1151 v2, Coﬀee Lake-S CPU

CPU vent: Freezer 13 from Arctic

SSD:V-NAND SSD 860 Pro Sata 6 Gb/s from Samsung [Size: 256 Gb]

HD: 2x 2000GB WD Red WD20EFAX 256MB 3.5“ (8.9cm) SATA 6Gb/s

RAM: 32GB G.Skill Aegis DDR4-3000 DIMM CL16 Dual Kit

NI-Card:

Serial Adapter:

Power supply unit: EVGA Supernova 530 G3

Computer chassis: Inter-Tech Case IPC Server 4U-4088-S

Drive drawer: LC-Power Festplattenadapter für 3.5” Festplatten (LC-ADA-525-35-SWAP)

Chassis vent: NB-BlackSilent PRO [120x120x25] from NoiseBlocker