TEC Service XY

Version: v3.00
Application: Meerstetter Control Software for ECDL baseplate, active shieldings of resonators R1 and R2.
Installation:

Copy folders with TEC Software

Set a software shortcut on the desktop

right click on each shortcut to change the “Ziel” and “Ausführen in”

R1 → DevAddr 1

R2 → DevAddr 2

ECDL Baseplate → DevAddr 0