Vacuum components

All CF-components are CF40!

Vacuum pump/controller/H.V. cable

Company: Agilent Technologies

Pump

Typ: VACION PLUS 40 STARCELL PUMP BASIC PUMP [Number: 9191240](http://www.agilent.com/en-us/products/vacuum-technologies/high-vacuum-pumps/ion-pumps/vacion-plus-40)

Catalog: agilent_catalog_06_ion_section_120.pdf

Manual: vacion_plus_40-55-75_pumps_user_manual.pdf

Heater for Medium VIP Instructions: heater_for_medium_vip_instructions.pdf

Auto Cad: http://www.agilent.com/cs/common/plusimages/VacIon-Plus-40-Ion-Pump-outline-drawing.png

Other informations: “Die einzigen Einflussgrößen auf die Stabilität des Druckes sind Gaslast und Ausgasung (eigentlich auch zur Gaslast gehörend).”

Controller

Typ: MINIVAC, FISCHER HV CONNECTOR, EUROPEAN PLUG 220V [Number: 9290290]

Manual: minivac_0190_1-0290_1_1_.pdf

H.V. cable

Typ: HV BAKEABLE CABLE, RADIATION RESISTANT, 13 (4 M) LONG WITH INTERLOCK FOR PUMPS CARRYING F/T [Number: 9290705]

Length: 4m

Datasheet/Manual: hv_radiation_resistant_cable_with_interlock-fischer_instructions.pdf

Grtound connection notice: This pump cable can be connected to the pump only after a separate ground connection (⇐0.1Ω) is made from pump body to the ground.

Vacuum sensor

Company: Pfeiffer Vacuum

Sensor

Typ: KR 270, metallgedichtet, DN 40 CF-F (Short version)(https://www.pfeiffer-vacuum.com/de/produkte/messgeraete/activeline/activeline-transmitter/?detailPdoId=3866)

Manual:

German: ikr270_cold-cathode_german.pdf

English: pfeiffer_cold_cath_gage_ikr_270_english.pdf

Auto Cad: https://static.pfeiffer-vacuum.com/productImages/de-DE/b01cee57-690b-11e6-80ca-005056950a30.png

Controller

Typ: TPG 261 (2008/12), No: PTG28030,F-No: 44308384

Datasheet/Manual: pfeiffer_single_gauge_tpg261.pdf

Cable

Typ: PT 448 250-T (https://www.pfeiffer-vacuum.com/de/produkte/messgeraete/activeline/activeline-transmitter/?detailPdoId=3381)

Length: 3m

Vacuum valves

Company: VAT

Gate valve

Typ: Mini UHV gate valve, Series 010, DN 40 (http://www.vatvalve.com/de/business/valves/product?id=01032-CE01)

Ordering No.: 01032-CE01

Datasheet: datasheet.pdf

Installation, Operating & Maintenance Instructions: installation_operating.pdf

Auto Cad (2D): gate_valve_2d.pdf

Angle valve

Typ: «Easy close» all-metal angle valve, Series 54 DN 40 (http://www.vatvalve.com/de/business/valves/product?id=54132-GE02)

Ordering No.: 54132-GE02-0001

Datasheet: datasheet_angle_valve.pdf

Installation, Operating & Maintenance Instructions: montageanleitung_angle_valve.pdf

Auto Cad (2D): ed_angle_valve.pdf

Other vacuum CF-components

Vacuum isolator

Test report scan copy for vacuum compatible isolators: test_report_scan_copy_for_vacuum_compatible_isolators.pdf