How to open the Vacuum

The Instruction is on AFS in the Magnesium Document folder, also on the wall nest to the vacumm controler.

belueftung_der_kammer.docx

We opened the Chamber on:

2015/12/17 Changed: Lattice Viewports, Zeeman Viewport

Indium sealing

You need

Clean surface and flat surface to press the window on