Todo

(Halb)Jährliches Todo

Wasserkühlung: Filter und Wasser wechseln (Letztes mal: März 16)

MOT-Spulen reinigen (warmes Essigwasser) (Letztes mal: April 16)

Notstromaggregat jährlich testen

Vorvakuumpumpenöl überprüfen bzw wechseln

To do till the end of January 2018

Long term ToDo plans

Clock laser fiber stabilization setup. How to do this for low clock laser powers?? - Discuss every week to finalize a setup plan.

Think of how to collimate clock laser with waist position at the atoms. - Discuss every week to finalize a plan soon.

Black body radiation uncertainty. - Discuss to decide what has to be done for 1 x 10^-17 uncertainty.

Measure magnetic field stabilities and their contribution to linewidth/accuracy. [N,W]

Crossed dipole trap for better loading into the lattice and for studying collisions.

Improvements in atom loading/spectroscopy sequence. (2018)

Dipole laser power dependence on atom numbers in lattice. (2018)

Allgemeine Probleme, die zu lösen sind

200A Current

Homg. B-Field

285

Triplet Laser

Wutz

Gitter